Best Management Practice Inspection Job Aid: Outlet Protection
This job aid is a tool to assist with the completion of Form 2118. All required corrective actions, comments, or discussions must be documented on Form 2118.
Review each criterion below. For each item, check the box or mark an “X” next to the appropriate response to indicate the compliance status: Yes (Y), No (N), or Not Applicable (NA) to indicate the compliance status.
Yes – The requirement has been met.
No – The requirement has not been met.
Not Applicable – The requirement does not apply to this project or site conditions.
Installation criteria
1) Are outlet protection controls documented in the Stormwater
Discharge Map or Erosion Control Sheets?	☐Y   ☐N   ☐NA
2) Are outlet protection controls installed in accordance with the
Stormwater Discharge Map or Erosion Control Sheets?	☐Y   ☐N   ☐NA
3) Were the outlet protection controls installed prior to construction
and or land disturbing activities?	☐Y   ☐N   ☐NA
4) Have the outlet protection controls been installed on all outlets 
where the design storm velocity exceeds 4 feet per second and 
discharges to an unlined or natural stream?	☐Y   ☐N   ☐NA
5) Is the riprap apron aligned with flow direction to minimize scour 
and erosion?	☐Y   ☐N   ☐NA
6) Is the slope on the apron equal to 0%?	☐Y   ☐N   ☐NA
7) Is the minimum apron length equal 4.5 times the outlet pipe
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diameter?	☐Y   ☐N   ☐NA
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8) Is the minimum apron width equal to 4.0 times the outlet 
pipe diameter?	☐Y   ☐N   ☐NA
9) Is the minimum apron depth equal to 1.5 times the maximum 
stone diameter?	☐Y   ☐N   ☐NA
10) Have design calculations been provided by the designer?	☐Y   ☐N   ☐NA
11) Has the riprap been placed to prevent damage to the underlying 
filter fabric?	☐Y   ☐N   ☐NA
Inspection criteria
1) Are the outlet protection controls functioning properly (for example,
no scour, standing water, or sediment buildup, etcetera)?	☐Y   ☐N   ☐NA
2) Is the underlaying fabric damaged?	☐Y   ☐N   ☐NA
3) Has there been any displacement of riprap?	☐Y   ☐N   ☐NA
4) Is the area surrounding the outlet protection free of scour?	☐Y   ☐N   ☐NA
5) Is the outfall clogged?	☐Y   ☐N   ☐NA
6) Do outlet protection controls impede traffic or cause flooding
and or standing water?	☐Y   ☐N   ☐NA
7) Were any concerns identified with the outlet protection?	☐Y   ☐N   ☐NA
8) Were maintenance requirements recommended to the contractor?	☐Y   ☐N   ☐NA
Maintenance criteria
1) Are the outlet protection controls in good condition without any 
visible damage?	☐Y   ☐N   ☐NA
2) Are associated Best Management Practices (BMPs) functioning 
properly?	☐Y   ☐N   ☐NA
3) Has the underlying fabric been replaced or repaired, if needed?	☐Y   ☐N   ☐NA
4) Have riprap been rekeyed in to prevent displacement, if needed?	☐Y   ☐N   ☐NA
5) Have outlet clogs or debris been removed, if any?	☐Y   ☐N   ☐NA
6) Have scour locations been repaired, if any?	☐Y   ☐N   ☐NA
7) Have adjustments been made to prevent traffic issues or flooding, 
if needed?	☐Y   ☐N   ☐NA
8) Has sediment been removed from the outlet protection control, 
if any?	☐Y   ☐N   ☐NA
9) Did the contractor address all recommended maintenance needs?	☐Y   ☐N   ☐NA
10) Were any additional BMPs recommended to the Contractor?	☐Y   ☐N   ☐NA
Comments and Notes
[Enter comments and notes]
Reference
Texas Pollutant Discharge Elimination System (TPDES) Construction General Permit TXR150000, Part III, Section F
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